{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":5,"n_cols":9,"rows_kept":5,"flags":["formulas_cached_only"]}
["Distributed Loads"]
[]
["Node A","Node B","Load","Ph-1","Ph-1","Ph-2","Ph-2","Ph-3","Ph-3"]
[null,null,"Model","kW","kVAr","kW","kVAr","kW","kVAr"]
[632,671,"Y-PQ",17,10,66,38,117,68]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}