{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":4,"rows_kept":16,"flags":["formulas_cached_only"]}
["Regulator Data"]
[]
["Regulator ID:",1]
["Line Segment:","650 - 632"]
["Location:",50]
["Phases:","A - B -C"]
["Connection:","3-Ph,LG"]
["Monitoring Phase:","A-B-C"]
["Bandwidth:","2.0 volts"]
["PT Ratio:",20]
["Primary CT Rating:",700]
["Compensator Settings:","Ph-A","Ph-B","Ph-C"]
["R - Setting:",3,3,3]
["X - Setting:",9,9,9]
["Volltage Level:",122,122,122]
["*********************************************************************"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}